(footprint "CM0"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Raspberry PI CM0 compute module")
	(tags "CM0 rpi raspberry pi compute module castellated")
	(property "Reference" "REF**"
		(at -3 -2 90)
		(layer "F.SilkS")
	)
	(property "Value" "CM0"
		(at 19.5 4.5 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" "Raspberry PI CM0 compute module"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 16.75 -20.5 0)
		(layer "F.Fab")
	)
	(pad "1" smd oval
		(at 0 -32.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at 0 -31.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at 0 -30.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at 0 -29.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at 0 -28.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at 0 -27.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at 0 -26.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at 0 -25.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at 0 -24.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at 0 -23.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at 0 -22.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at 0 -21.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at 0 -20.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at 0 -19.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at 0 -18.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at 0 -17.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd oval
		(at 0 -16.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd oval
		(at 0 -15.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd oval
		(at 0 -14.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd oval
		(at 0 -13.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd oval
		(at 0 -12.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd oval
		(at 0 -11.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd oval
		(at 0 -10.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd oval
		(at 0 -9.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd oval
		(at 0 -8.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd oval
		(at 0 -7.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd oval
		(at 0 -6.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd oval
		(at 0 -5.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd oval
		(at 0 -4.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd oval
		(at 0 -3.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd oval
		(at 0 -2.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd oval
		(at 0 -1.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd oval
		(at 0 -0.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd oval
		(at 3.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd oval
		(at 4.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd oval
		(at 5.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd oval
		(at 6.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd oval
		(at 7.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd oval
		(at 8.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd oval
		(at 9.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd oval
		(at 10.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd oval
		(at 11.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd oval
		(at 12.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd oval
		(at 13.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd oval
		(at 14.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd oval
		(at 15.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd oval
		(at 16.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd oval
		(at 17.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd oval
		(at 18.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd oval
		(at 19.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd oval
		(at 20.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd oval
		(at 21.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd oval
		(at 22.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd oval
		(at 23.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd oval
		(at 24.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd oval
		(at 25.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd oval
		(at 26.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd oval
		(at 27.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd oval
		(at 28.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd oval
		(at 29.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd oval
		(at 30.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd oval
		(at 31.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd oval
		(at 32.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd oval
		(at 33.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd oval
		(at 34.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd oval
		(at 35.5 0 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd oval
		(at 39 -0.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd oval
		(at 39 -1.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd oval
		(at 39 -2.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd oval
		(at 39 -3.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd oval
		(at 39 -4.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd oval
		(at 39 -5.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd oval
		(at 39 -6.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd oval
		(at 39 -7.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd oval
		(at 39 -8.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "76" smd oval
		(at 39 -9.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "77" smd oval
		(at 39 -10.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "78" smd oval
		(at 39 -11.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "79" smd oval
		(at 39 -12.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "80" smd oval
		(at 39 -13.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "81" smd oval
		(at 39 -14.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "82" smd oval
		(at 39 -15.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "83" smd oval
		(at 39 -16.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "84" smd oval
		(at 39 -17.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "85" smd oval
		(at 39 -18.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "86" smd oval
		(at 39 -19.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "87" smd oval
		(at 39 -20.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "88" smd oval
		(at 39 -21.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "89" smd oval
		(at 39 -22.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "90" smd oval
		(at 39 -23.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "91" smd oval
		(at 39 -24.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "92" smd oval
		(at 39 -25.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "93" smd oval
		(at 39 -26.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "94" smd oval
		(at 39 -27.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "95" smd oval
		(at 39 -28.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "96" smd oval
		(at 39 -29.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "97" smd oval
		(at 39 -30.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "98" smd oval
		(at 39 -31.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "99" smd oval
		(at 39 -32.5)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "100" smd oval
		(at 35.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "101" smd oval
		(at 34.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "102" smd oval
		(at 33.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "103" smd oval
		(at 32.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "104" smd oval
		(at 31.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "105" smd oval
		(at 30.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "106" smd oval
		(at 29.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "107" smd oval
		(at 28.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "108" smd oval
		(at 27.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "109" smd oval
		(at 26.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "110" smd oval
		(at 25.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "111" smd oval
		(at 24.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "112" smd oval
		(at 23.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "113" smd oval
		(at 22.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "114" smd oval
		(at 21.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "115" smd oval
		(at 20.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "116" smd oval
		(at 19.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "117" smd oval
		(at 18.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "118" smd oval
		(at 17.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "119" smd oval
		(at 16.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "120" smd oval
		(at 15.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "121" smd oval
		(at 14.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "122" smd oval
		(at 13.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "123" smd oval
		(at 12.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "124" smd oval
		(at 11.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "125" smd oval
		(at 10.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "126" smd oval
		(at 9.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "127" smd oval
		(at 8.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "128" smd oval
		(at 7.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "129" smd oval
		(at 6.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "130" smd oval
		(at 5.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "131" smd oval
		(at 4.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "132" smd oval
		(at 3.5 -33 90)
		(size 2.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "CM0_3D_simple.step")
			(type model)
		)
	)
	(model "kicad-embed://CM0_3D_simple.step"
		(offset (xyz 0 0 0))
		(scale (xyz 1 1 1))
		(rotate (xyz 0 0 0))
	)
)
