(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CM0"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -2.54 0)
		)
		(property "Value" "CM0"
			(at 0 2.54 0)
		)
		(property "Footprint" "Raspberrypi_cm0:CM0"
			(at 0 0 0)
		)
		(property "Datasheet" "https://opcenter.de/pub/misc/cm0+cm0-dev-board-datasheet-en_retranslated.pdf#page=12"
			(at 0 0 0)
		)
		(property "Description" "RaspberryPi CM0 compute module"
			(at 0 0 0)
		)
		(symbol "CM0_1_0")
		(symbol "CM0_1_1"
			(pin passive line
				(at -60.96 40.64 0)
				(length 7.62)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at -60.96 38.1 0)
				(length 7.62)
				(name "DSI_D3_P")
				(number "2")
			)
			(pin output line
				(at -60.96 35.56 0)
				(length 7.62)
				(name "DSI_D3_N")
				(number "3")
			)
			(pin passive line
				(at -60.96 33.02 0)
				(length 7.62)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at -60.96 30.48 0)
				(length 7.62)
				(name "DSI_D2_P")
				(number "5")
			)
			(pin output line
				(at -60.96 27.94 0)
				(length 7.62)
				(name "DSI_D2_N")
				(number "6")
			)
			(pin passive line
				(at -60.96 25.4 0)
				(length 7.62)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at -60.96 22.86 0)
				(length 7.62)
				(name "DSI_CL_P")
				(number "8")
			)
			(pin output line
				(at -60.96 20.32 0)
				(length 7.62)
				(name "DSI_CK_N")
				(number "9")
			)
			(pin passive line
				(at -60.96 17.78 0)
				(length 7.62)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at -60.96 15.24 0)
				(length 7.62)
				(name "DSI_D1_P")
				(number "11")
			)
			(pin output line
				(at -60.96 12.7 0)
				(length 7.62)
				(name "DSI_D1_N")
				(number "12")
			)
			(pin passive line
				(at -60.96 10.16 0)
				(length 7.62)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at -60.96 7.62 0)
				(length 7.62)
				(name "DSI_D0_P")
				(number "14")
			)
			(pin output line
				(at -60.96 5.08 0)
				(length 7.62)
				(name "DSI_D0_N")
				(number "15")
			)
			(pin passive line
				(at -60.96 2.54 0)
				(length 7.62)
				(name "GND")
				(number "16")
			)
			(pin input line
				(at -60.96 0 0)
				(length 7.62)
				(name "HDMI_HPD")
				(number "17")
			)
			(pin bidirectional line
				(at -60.96 -2.54 0)
				(length 7.62)
				(name "HDMI_SDA")
				(number "18")
			)
			(pin bidirectional line
				(at -60.96 -5.08 0)
				(length 7.62)
				(name "HDMI_SCL")
				(number "19")
			)
			(pin input line
				(at -60.96 -7.62 0)
				(length 7.62)
				(name "HDMI_CEC")
				(number "20")
			)
			(pin passive line
				(at -60.96 -10.16 0)
				(length 7.62)
				(name "GND")
				(number "21")
			)
			(pin output line
				(at -60.96 -12.7 0)
				(length 7.62)
				(name "HDMI_CK_N")
				(number "22")
			)
			(pin output line
				(at -60.96 -15.24 0)
				(length 7.62)
				(name "HDMI_CK_P")
				(number "23")
			)
			(pin passive line
				(at -60.96 -17.78 0)
				(length 7.62)
				(name "GND")
				(number "24")
			)
			(pin output line
				(at -60.96 -20.32 0)
				(length 7.62)
				(name "HDMI_D0_N")
				(number "25")
			)
			(pin output line
				(at -60.96 -22.86 0)
				(length 7.62)
				(name "HDMI_D0_P")
				(number "26")
			)
			(pin passive line
				(at -60.96 -25.4 0)
				(length 7.62)
				(name "GND")
				(number "27")
			)
			(pin output line
				(at -60.96 -27.94 0)
				(length 7.62)
				(name "HDMI_D1_N")
				(number "28")
			)
			(pin output line
				(at -60.96 -30.48 0)
				(length 7.62)
				(name "HDMI_D1_P")
				(number "29")
			)
			(pin passive line
				(at -60.96 -33.02 0)
				(length 7.62)
				(name "GND")
				(number "30")
			)
			(pin output line
				(at -60.96 -35.56 0)
				(length 7.62)
				(name "HDMI_D2_N")
				(number "31")
			)
			(pin output line
				(at -60.96 -38.1 0)
				(length 7.62)
				(name "HDMI_D2_P")
				(number "32")
			)
			(pin passive line
				(at -60.96 -40.64 0)
				(length 7.62)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at -40.64 53.34 270)
				(length 7.62)
				(name "GND")
				(number "132")
			)
			(pin passive line
				(at -40.64 -53.34 90)
				(length 7.62)
				(name "GND")
				(number "34")
			)
			(pin bidirectional line
				(at -38.1 53.34 270)
				(length 7.62)
				(name "SD_DAT2")
				(number "131")
			)
			(pin bidirectional line
				(at -38.1 -53.34 90)
				(length 7.62)
				(name "USB_N")
				(number "35")
			)
			(pin bidirectional line
				(at -35.56 53.34 270)
				(length 7.62)
				(name "SD_DAT3")
				(number "130")
			)
			(pin tri_state line
				(at -35.56 -53.34 90)
				(length 7.62)
				(name "USB_P")
				(number "36")
			)
			(pin passive line
				(at -33.02 53.34 270)
				(length 7.62)
				(name "GND")
				(number "129")
			)
			(pin passive line
				(at -33.02 -53.34 90)
				(length 7.62)
				(name "GND")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 53.34 270)
				(length 7.62)
				(name "SD_CMD")
				(number "128")
			)
			(pin input line
				(at -30.48 -53.34 90)
				(length 7.62)
				(name "USB_OTG")
				(number "38")
			)
			(pin output line
				(at -27.94 53.34 270)
				(length 7.62)
				(name "SD_CLK")
				(number "127")
			)
			(pin output line
				(at -27.94 -53.34 90)
				(length 7.62)
				(name "CVBS")
				(number "39")
			)
			(pin passive line
				(at -25.4 53.34 270)
				(length 7.62)
				(name "GND")
				(number "126")
			)
			(pin passive line
				(at -25.4 -53.34 90)
				(length 7.62)
				(name "GND")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 53.34 270)
				(length 7.62)
				(name "SD_DAT0")
				(number "125")
			)
			(pin power_out line
				(at -22.86 -53.34 90)
				(length 7.62)
				(name "CM0_3.3V")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 53.34 270)
				(length 7.62)
				(name "SD_DAT1")
				(number "124")
			)
			(pin bidirectional line
				(at -20.32 -53.34 90)
				(length 7.62)
				(name "SDA0")
				(number "42")
			)
			(pin passive line
				(at -17.78 53.34 270)
				(length 7.62)
				(name "GND")
				(number "123")
			)
			(pin bidirectional line
				(at -17.78 -53.34 90)
				(length 7.62)
				(name "SCL0")
				(number "43")
			)
			(pin input line
				(at -15.24 53.34 270)
				(length 7.62)
				(name "SD_VREF")
				(number "122")
			)
			(pin bidirectional line
				(at -15.24 -53.34 90)
				(length 7.62)
				(name "CAM_GPIO")
				(number "44")
			)
			(pin input line
				(at -12.7 53.34 270)
				(length 7.62)
				(name "RPI_BOOT")
				(number "121")
			)
			(pin passive line
				(at -12.7 -53.34 90)
				(length 7.62)
				(name "GND")
				(number "45")
			)
			(pin power_out line
				(at -10.16 53.34 270)
				(length 7.62)
				(name "CM0_3.3V")
				(number "120")
			)
			(pin input line
				(at -10.16 -53.34 90)
				(length 7.62)
				(name "CSI_D3_P")
				(number "46")
			)
			(pin power_out line
				(at -7.62 53.34 270)
				(length 7.62)
				(name "CM0_3.3V")
				(number "119")
			)
			(pin input line
				(at -7.62 -53.34 90)
				(length 7.62)
				(name "CSI_D3_N")
				(number "47")
			)
			(pin output line
				(at -5.08 53.34 270)
				(length 7.62)
				(name "LED_nACT")
				(number "118")
			)
			(pin passive line
				(at -5.08 -53.34 90)
				(length 7.62)
				(name "GND")
				(number "48")
			)
			(pin input line
				(at -2.54 53.34 270)
				(length 7.62)
				(name "BT_ON")
				(number "117")
			)
			(pin input line
				(at -2.54 -53.34 90)
				(length 7.62)
				(name "CSI_D2_P")
				(number "49")
			)
			(pin input line
				(at 0 53.34 270)
				(length 7.62)
				(name "WiFi_ON")
				(number "116")
			)
			(pin input line
				(at 0 -53.34 90)
				(length 7.62)
				(name "CSI_D2_N")
				(number "50")
			)
			(pin passive line
				(at 2.54 53.34 270)
				(length 7.62)
				(name "GND")
				(number "115")
			)
			(pin passive line
				(at 2.54 -53.34 90)
				(length 7.62)
				(name "GND")
				(number "51")
			)
			(pin bidirectional line
				(at 5.08 53.34 270)
				(length 7.62)
				(name "GPIO2")
				(number "114")
			)
			(pin input line
				(at 5.08 -53.34 90)
				(length 7.62)
				(name "CSI_CK_P")
				(number "52")
			)
			(pin bidirectional line
				(at 7.62 53.34 270)
				(length 7.62)
				(name "GPIO3")
				(number "113")
			)
			(pin input line
				(at 7.62 -53.34 90)
				(length 7.62)
				(name "CSI_CK_N")
				(number "53")
			)
			(pin passive line
				(at 10.16 53.34 270)
				(length 7.62)
				(name "GND")
				(number "112")
			)
			(pin passive line
				(at 10.16 -53.34 90)
				(length 7.62)
				(name "GND")
				(number "54")
			)
			(pin bidirectional line
				(at 12.7 53.34 270)
				(length 7.62)
				(name "GPIO4")
				(number "111")
			)
			(pin input line
				(at 12.7 -53.34 90)
				(length 7.62)
				(name "CSI_D1_P")
				(number "55")
			)
			(pin bidirectional line
				(at 15.24 53.34 270)
				(length 7.62)
				(name "GPIO14")
				(number "110")
			)
			(pin input line
				(at 15.24 -53.34 90)
				(length 7.62)
				(name "CSI_D1_N")
				(number "56")
			)
			(pin passive line
				(at 17.78 53.34 270)
				(length 7.62)
				(name "GND")
				(number "109")
			)
			(pin passive line
				(at 17.78 -53.34 90)
				(length 7.62)
				(name "GND")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 53.34 270)
				(length 7.62)
				(name "GPIO15")
				(number "108")
			)
			(pin input line
				(at 20.32 -53.34 90)
				(length 7.62)
				(name "CSI_D0_P")
				(number "58")
			)
			(pin bidirectional line
				(at 22.86 53.34 270)
				(length 7.62)
				(name "GPIO17")
				(number "107")
			)
			(pin input line
				(at 22.86 -53.34 90)
				(length 7.62)
				(name "CSI_D0_N")
				(number "59")
			)
			(pin passive line
				(at 25.4 53.34 270)
				(length 7.62)
				(name "GND")
				(number "106")
			)
			(pin passive line
				(at 25.4 -53.34 90)
				(length 7.62)
				(name "GND")
				(number "60")
			)
			(pin bidirectional line
				(at 27.94 53.34 270)
				(length 7.62)
				(name "GPIO18")
				(number "105")
			)
			(pin bidirectional line
				(at 27.94 -53.34 90)
				(length 7.62)
				(name "RUN_PG")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 53.34 270)
				(length 7.62)
				(name "GPIO27")
				(number "104")
			)
			(pin input line
				(at 30.48 -53.34 90)
				(length 7.62)
				(name "GLOBAL_EN")
				(number "62")
			)
			(pin passive line
				(at 33.02 53.34 270)
				(length 7.62)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at 33.02 -53.34 90)
				(length 7.62)
				(name "GND")
				(number "63")
			)
			(pin bidirectional line
				(at 35.56 53.34 270)
				(length 7.62)
				(name "GPIO22")
				(number "102")
			)
			(pin power_out line
				(at 35.56 -53.34 90)
				(length 7.62)
				(name "CM0_1.8V")
				(number "64")
			)
			(pin bidirectional line
				(at 38.1 53.34 270)
				(length 7.62)
				(name "GPIO23")
				(number "101")
			)
			(pin power_out line
				(at 38.1 -53.34 90)
				(length 7.62)
				(name "CM0_1.8V")
				(number "65")
			)
			(pin passive line
				(at 40.64 53.34 270)
				(length 7.62)
				(name "GND")
				(number "100")
			)
			(pin passive line
				(at 40.64 -53.34 90)
				(length 7.62)
				(name "GND")
				(number "66")
			)
			(pin passive line
				(at 60.96 40.64 180)
				(length 7.62)
				(name "GND")
				(number "99")
			)
			(pin bidirectional line
				(at 60.96 38.1 180)
				(length 7.62)
				(name "GPIO24")
				(number "98")
			)
			(pin bidirectional line
				(at 60.96 35.56 180)
				(length 7.62)
				(name "GPIO10")
				(number "97")
			)
			(pin passive line
				(at 60.96 33.02 180)
				(length 7.62)
				(name "GND")
				(number "96")
			)
			(pin bidirectional line
				(at 60.96 30.48 180)
				(length 7.62)
				(name "GPIO9")
				(number "95")
			)
			(pin bidirectional line
				(at 60.96 27.94 180)
				(length 7.62)
				(name "GPIO25")
				(number "94")
			)
			(pin passive line
				(at 60.96 25.4 180)
				(length 7.62)
				(name "GND")
				(number "93")
			)
			(pin bidirectional line
				(at 60.96 22.86 180)
				(length 7.62)
				(name "GPIO11")
				(number "92")
			)
			(pin bidirectional line
				(at 60.96 20.32 180)
				(length 7.62)
				(name "GPIO8")
				(number "91")
			)
			(pin passive line
				(at 60.96 17.78 180)
				(length 7.62)
				(name "GND")
				(number "90")
			)
			(pin bidirectional line
				(at 60.96 15.24 180)
				(length 7.62)
				(name "GPIO7")
				(number "89")
			)
			(pin bidirectional line
				(at 60.96 12.7 180)
				(length 7.62)
				(name "ID_SD")
				(number "88")
			)
			(pin passive line
				(at 60.96 10.16 180)
				(length 7.62)
				(name "GND")
				(number "87")
			)
			(pin bidirectional line
				(at 60.96 7.62 180)
				(length 7.62)
				(name "ID_SC")
				(number "86")
			)
			(pin bidirectional line
				(at 60.96 5.08 180)
				(length 7.62)
				(name "GPIO5")
				(number "85")
			)
			(pin passive line
				(at 60.96 2.54 180)
				(length 7.62)
				(name "GND")
				(number "84")
			)
			(pin bidirectional line
				(at 60.96 0 180)
				(length 7.62)
				(name "GPIO6")
				(number "83")
			)
			(pin bidirectional line
				(at 60.96 -2.54 180)
				(length 7.62)
				(name "GPIO12")
				(number "82")
			)
			(pin passive line
				(at 60.96 -5.08 180)
				(length 7.62)
				(name "GND")
				(number "81")
			)
			(pin bidirectional line
				(at 60.96 -7.62 180)
				(length 7.62)
				(name "GPIO13")
				(number "80")
			)
			(pin bidirectional line
				(at 60.96 -10.16 180)
				(length 7.62)
				(name "GPIO19")
				(number "79")
			)
			(pin passive line
				(at 60.96 -12.7 180)
				(length 7.62)
				(name "GND")
				(number "78")
			)
			(pin bidirectional line
				(at 60.96 -15.24 180)
				(length 7.62)
				(name "GPIO16")
				(number "77")
			)
			(pin bidirectional line
				(at 60.96 -17.78 180)
				(length 7.62)
				(name "GPIO26")
				(number "76")
			)
			(pin passive line
				(at 60.96 -20.32 180)
				(length 7.62)
				(name "GND")
				(number "75")
			)
			(pin bidirectional line
				(at 60.96 -22.86 180)
				(length 7.62)
				(name "GPIO20")
				(number "74")
			)
			(pin bidirectional line
				(at 60.96 -25.4 180)
				(length 7.62)
				(name "GPIO21")
				(number "73")
			)
			(pin passive line
				(at 60.96 -27.94 180)
				(length 7.62)
				(name "GND")
				(number "72")
			)
			(pin unspecified line
				(at 60.96 -30.48 180)
				(length 7.62)
				(hide yes)
				(name "NC")
				(number "71")
			)
			(pin unspecified line
				(at 60.96 -33.02 180)
				(length 7.62)
				(hide yes)
				(name "NC")
				(number "70")
			)
			(pin passive line
				(at 60.96 -35.56 180)
				(length 7.62)
				(name "GND")
				(number "69")
			)
			(pin power_in line
				(at 60.96 -38.1 180)
				(length 7.62)
				(name "5V")
				(number "68")
			)
			(pin power_in line
				(at 60.96 -40.64 180)
				(length 7.62)
				(name "5V")
				(number "67")
			)
		)
		(embedded_fonts no)
	)
)
